|  |  |  |
| --- | --- | --- |
| PINION TOOTH COUNT | CROWNWHEEL TOOTH COUNT | RATIO  |
|  |  |  |
| 9 | 40 | 4.44:1 |
|  |  |  |
| 8 | 33 | 4.125:1 |
|  |  |  |
| 9 | 35 | 3.889 |
|  |  |  |
| 9 | 34 | 3.777 |
|  |  |  |
| 11 | 39 | 3.54 |

Other useful information taken from Ford workshop manual

OIL CAPACITY 1.1 Litres (approx)

OIL GRADE SAE 90 HYPOID

CW&P BACKLASH 0.005 to 0.007 in. (0.13 to 0.18mm)